**Parts and Tools List for Constructing and Launching a SSR**

List of parts for one SSR kit:

* One big bertha kit
* X1 Eyebolt
* x2 washers
* x2 nuts
* x3 1” screws for bulkhead
* x4 1/4-1/2” screws for nosecone
* x3 bulkhead #12219
* x1 centering ring #13416
* Kevlar shock chord
* x1 Dynochute  36"
* x1 parachute swivel #29621
* x1 parachute hook #14510
* clamps(optional for fins and bulkhead)

Tools for construction:

* drill with 1/8” drill bit
* long needle nose pliers
* exacto or hobby knife
* scissors
* hacksaw to cut nosecone
* screwdriver

Tools for launch:

* long needle nose
* screwdriver
* scissors

Consumables:

* wood glue
* super glue
* two part epoxy
* Spray Paint
* Duct Tape

Prepared by Lee Bequette