Post Launch Procedure

Disconnect battery

Extinguish any fires

Recover rocket(s)

Disarm electronics

Launch site disassembly

Store all launch equipment in appropriate area

Complete launch log

Store un-used motors in fireproof cabinet

Ensure all batteries are disconnected

Collect all flight data and videos/pictures

Dunk used motors in water and dispose

Ensure electronics are stored properly

Conduct after action report